# jan/02/1970 21:56:15 by RouterOS 6.47.8
# software id = Z8UP-HFV6
#
# model = RB750Gr3
# serial number = D5030D16428C
/interface bridge
add name=LAN_INET
add name="loopback Monitoreo"
/interface wireless security-profiles
set [ find default=yes ] supplicant-identity=MikroTik
/ip hotspot profile
set [ find default=yes ] html-directory=flash/hotspot
/snmp community
add addresses=190.61.4.34/32,190.61.4.170/32,190.61.4.35/32 name=ifxcliente write-access=yes
/interface bridge port
add bridge=LAN_INET interface=ether2
add bridge=LAN_INET interface=ether3
add bridge=LAN_INET interface=ether4
add bridge=LAN_INET interface=ether5
/ip address
add address=10.220.5.238/30 interface=ether1 network=10.220.5.236
add address=190.115.0.37/24 interface=LAN_INET network=190.115.0.0
/ip route
add distance=1 gateway=10.220.5.237
/ip service
set telnet disabled=yes
set ftp disabled=yes
set www disabled=yes
set ssh address=190.60.0.0/16,190.61.0.0/16,172.16.0.0/16,172.17.0.0/16,10.0.120.0/24,200.62.0.0/16,200.91.0.0/16,181.53.13.26/32,200.78.196.69/32
set winbox address=190.60.0.0/16,200.62.0.0/16,200.91.0.0/16,181.53.13.26/32
/snmp
set enabled=yes trap-community=ifxcliente
/system identity
set name=SID_1459324_TRANSPORTE_ADMIN_VALORES_TECULUTAN